**Name of Stakeholder:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

| **Section** | **Original Provision** | **Proposed Amendment** | **Rationale** | **Comments/Proposed Revision**  | **Rationale** |
| --- | --- | --- | --- | --- | --- |
| ***Procedures During Test and Commissioning*** | xxx xxx xxx* + 1. Immediately upon expiry of the Provisional CATC or upon certification that the Generation Facility has completed the conduct of Test and Commissioning, the following shall be observed:
1. The SO shall cease submission of over-riding constraints to the MO to prevent continuous injection of the Generation Facility while awaiting approval to commence Commercial Operations.
2. Should energy injections still be recorded from the Generation Facility, the Generation Company shall not be allowed to declare any bilateral contract quantity and shall not be entitled to any WESM payments for any injected energy but shall be charged for any energy withdrawn from the grid or distribution network. The TNP or the DU in case of Embedded Generator shall immediately cause the disconnection of the Generation Company to prevent further injection in the grid or distribution network.

xxx xxx xxx | xxx xxx xxx* + 1. Immediately upon expiry of the Provisional CATC or upon certification that the Generation Facility has completed the conduct of Test and Commissioning, the following shall be observed:
1. The SO shall cease submission of over-riding constraints to the MO to prevent continuous injection of the Generation Facility while awaiting approval to commence Commercial Operations.
2. Should energy injections still be recorded from the Generation Facility, the Generation Company shall not be allowed to declare any bilateral contract quantity and shall not be entitled to any WESM payments for any injected energy but shall be charged for any energy withdrawn from the grid or distribution network. The TNP or the DU in case of Embedded Generator shall immediately cause the disconnection of the Generation Company to prevent further injection in the grid or distribution network.

***Prior to the issuance of a COC by the ERC, a generation company that has been issued with a FCATC may be allowed to continue to operate and be compensated as price taker in the market, unless the ERC issues an Order for the generation company's immediate disconnection from the grid.***xxx xxx xxx | To maximize available power generating capacity at all times |  |  |